1. ALL DIMESIONS ARE IN MILLIMETERS EXCEPT THE
   PLANT CO-ORDINATES AND ELEVATIONS ARE IN METER.



2. PLANT ELEVATION DATUM EL.(+)100.000 M
   = 10 M (BALTIC SEA LEVEL)



3. ALL STRUCTURAL STEEL SHALL BE FABRICATED SM490A OF JISG3101.
   NOW STRUCTURAL MEMBER (SUCH AS HANDRAIL, LADDER, GRATING,
   CHEQUERED PLATE) SHALL BE FABRICATED WITH SS400 OF JISG3101.




4. FOR LADDER FOUNDATION RC DETAILS REFER STANDARD
   DRAWING NO. STD-TACE-001-CV-005



5. ALL VERTICAL BRACING CONNECTIONS ARE AS PER
    DWG.NO.STD-TACE-001-CV-011,012 & 013 (U.O.N.)



6.ALL PLAN BRACING CONNECTIONS ARE AS PER 
   DWG. NO.STD-TACE-001-CV-010 (U.O.N.)